Lecture 1

* Routing
  + Paths
* Data Links – physical layer
  + Between 2 nodes (error detection, etc.)
* Narrow physical layer restriction:
  + Need to send data in small bits
* DNS – directory service -> name to ip address
* Network header
  + Routing info (all intermediary routers)
* Data link header
  + Only info about next router
* Physical layer
  + No header, splits DPDU (?) (frame) into bits
* At destination node, data link header is taken off, then the network header. Then, it sees final destination is this router and proceeds to take off other headers
* Data links – fiber, wireless, cable, Bluetooth, etc.
* TCP vs. UDP transport layer
  + UDP – no resending/retransmission
  + TCP – more reliable
* TCP abstraction
  + Sender and receiver have 2 connected queues and data reliably is sent from sender to receiver queue. No packets.
  + Uses data link to send packets between 2 routers, which sends bits at physical layer

Lecture 2

* TCP
  + Queue abstraction
* IP layer
  + IP header places source and destination
  + If IP addresses match, then we are at the right destination
  + Else, figure out the next router
* Data link
  + From mac address x to y
* Mac address
  + Unique 48 bit addresses uniquely identify everyone on a link
  + E.g., x->y z->l, y,z are mac addresses for the same router
* IP address
  + Temporarily assigned to device
* Physical
  + Bits
* RPC (remote procedure calls) vs TCP (Queue abstraction)
* Socket = queue
* Transmission
  + Bandwidth
    - Range of frequencies a particular signal is created from (infinite sum of which sine wave freqs)
  + Strict layering
    - Only read headers at current layer (e.g., IP only reads IP header)
    - Information can only be passed across interfaces
  + Physical layer
    - Frequency shifting vs amplitude shifting (baseband)
    - Bits to coded bits to add transitions
    - Send bits to modem to convert to energy
  + Channel
    - Physical medium to transmit from sender to receiver
    - A channel does not change frequency of sine waves (only maybe the amplitude and phase)
  + Any periodic function can be written as an infinite sum of sin waves with diff freqs
  + More harmonics/bandwidth -> better bit recovery
  + Harmonic = multiple of the fundamental frequency
  + Channels are sluggish (take time to respond to a change in the signal)
  + Channels have noise, resulting in a change in amplitude
  + Sample at middle points
  + Two limits
    - Bandwidth (Nyquist rate) – limit on symbols (signals)
      * Input: square wave, output: falling sine wave
        + When can be send the second signal such that it does not interfere with previous signal?

Bandwidth of input signal is 1/T

You can theoretically send signals every T/2 seconds (Send at frequency: 2 \* bandwidth = 2/T)

Max rate of sending symbols, not bits (baud rate)

* + - * Why not send multiple bits per symbol (6v – 11, 4v – 10, …)
        + Noise
    - Noise (Shannon) – limit on bits
      * Maximum number of noise to tolerate to distinguish 6V and 4V is 1V, which limits the number of bits per symbol
      * Shannon limit applies to any channel (wire, wireless, etc.)
      * S – max signal
      * N – noise
      * Signals must be spaced 2\*N
      * B – bandwidth
      * Shannon limit is B \* log (1 + S/2N) bits per second